**TURNER HYDRAULIC SITE SERVICES**

Speed control 0-60 HZ, fully turned to left is Zero HZ

Pump on/off control



Suction Isolation Valve – always start in Open position.

Under Tank

Pump Bleed Plug

Outlet Isolation Valve – always start in closed position, then open slowly

Heater on / off switch, once on automatic control via above temperature controller

Temperature control set at 50°c